<?xml version="1.0" encoding="UTF-8" standalone="no"?>
<configurations XML_version="1.2" id="configurations_0">
    
<configuration XML_version="1.2" id="Texas Instruments XDS100v1 USB Debug Probe_0">
        <instance XML_version="1.2" desc="Texas Instruments XDS100v1 USB Debug Probe_0" href="connections/TIXDS100usb_Connection.xml" id="Texas Instruments XDS100v1 USB Debug Probe_0" xml="TIXDS100usb_Connection.xml" xmlpath="connections"/>
        <connection XML_version="1.2" id="Texas Instruments XDS100v1 USB Debug Probe_0">
            <instance XML_version="1.2" href="drivers/tixds100icepick_d.xml" id="drivers" xml="tixds100icepick_d.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds100c66xx.xml" id="drivers" xml="tixds100c66xx.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds100cs_dap.xml" id="drivers" xml="tixds100cs_dap.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds100csstm.xml" id="drivers" xml="tixds100csstm.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds100etbcs.xml" id="drivers" xml="tixds100etbcs.xml" xmlpath="drivers"/>
            <platform XML_version="1.2" id="platform_0">
                <instance XML_version="1.2" desc="TMS320C6678_0" href="devices/C6678.xml" id="TMS320C6678_0" xml="C6678.xml" xmlpath="devices"/>
            </platform>
        </connection>
    </configuration>
</configurations>
